Release Information

App (setup.exe) Version:V1.0.0.0 [11-06-2002]
App (DRemover.exe) Version: V1.3.0.1
Driver Version for Win98 & Me: V1.5.0.0
Driver Version for Win2K/XP: V1.5.0.5
Released date: 11/11/2002

Files Included in This Release:
	Setup.exe
	DRemover.exe
	readme.txt
	serwpl.inf
	Win98_ME\ser9pl.sys
	Win98_ME\serspl.inf
	Win98_ME\serspl.vxd
	Win2K\ser2pl.sys
		
Changes in this Release:
	None (First Rel.)
	
Note:   1. The USB-DC can only be used on a 500mA USB-Port. 
	   	Operation on a 100mA port may cause undesired results including system instability and loss of data.
	   	100 mA Port: PWR-LED and charging are deactivated automatically.
	   
	2. On WindowsXP: The installation via 'Setup.exe' is not supported. Please use the hardware assistant to 
		install the driver.
	
	3. After installation of the USB data cable driver and pluged-in data cable, a virtual COM port will be 
		generated. The name/ index of the allocated COM port can be accessed via the 'Device Manager'. 

	4. For deinstallation, after installation via 'setup.exe', please use the Control Panel - Add/Remove Program.

	5. After installation via Hardware Assistant the driver is not visible in the Control Panel. 
		Use for deinstallation the file 'DRemover.exe', stored on the driver CD.

	6. On Windows98SE: 'Suspend Mode'/'Stand by' is not supported during datatransfer.
	   	On Windows ME: 'Suspend Mode'/'Stand by' is not supported in general.

	7. In case of any COM-port allocation conflict (e.g. with an onboard modem), 
		choose a higher COM port (e.g. above port 10) via 'Device Manager' for the USB data cable.

-------------------------------------------------------------------------------------------------------


Information sur ce release

Version de l'appl. (setup.exe) : V1.0.0.0 [11-06-2002]
Version de l'appl. (DRemover) : V1.3.0.1
Version du pilote pour Win98 & Me : V1.5.0.0
Version du pilote pour Win2K/XP: V1.5.0.5
Date du release : 11/11/2002

Fichiers inclus dans ce release :
	Setup.exe
	DRemover.exe
	readme.txt
	serwpl.inf
	Win98_ME\ser9pl.sys
	Win98_ME\serspl.inf
	Win98_ME\serspl.vxd
	Win2K\ser2pl.sys
		
Changements de ce release :
	Aucun (premier rel.)
	
Rem. :  1. L'USB-DC peut uniquement s'utiliser sur un port USB 500mA. 
	   	Toute utilisation sur un port 100mA peut provoquer des effets non désirés dont une instabilité du système 		et des pertes de données.
	   	Port 100 mA : la DEL PWR et le chargement sont désactivés automatiquement.
	   
	2. Sous WindowsXP : l'installation via 'Setup.exe' n'est pas supportée. Utilisez l'Assistant Matériel pour 
		installer le pilote.
	
	3. Une fois l'installation du pilote du câble de données USB réalisée et le câble de données enfiché, un port COM 		virtuel est créé. Le nom/ index du port COM attribué est visible dans le 'Gestionnaire de 					périphériques'. 

	4. Pour désinstaller un pilote installé avec 'setup.exe', utilisez le Panneau de configuration - 					Ajout/Suppression de programmes.

	5. Après une installation avec l'Assistant Matériel, le pilote n'apparaît pas dans le Panneau de configuration. 			Pour le désinstaller, utilisez le fichier 'DRemover98_2K.exe' sur le CD de pilotes.

	6. Sous Windows98SE : le mode 'Suspend'/'Stand by' n'est pas supporté pendant le transfert de données.
		Sous Windows ME : le mode 'Suspend'/'Stand by' n'est pas supporté en général.

	7. En cas de conflit d'attribution du port COM (par exemple avec un modem intégré), 
		sélectionner pour le câble de données USB un port COM plus élevé (par exemple supérieur au port 10) 
		à l'aide du "Gestionnaire de périphériques".	

	
