Release Information

App (setup.exe) Version: V4.0.100 (04/15/2003)
App (DRemover98_2K.exe) Version: V1.3.0.1 (12/06/2002)
Driver Version for Win98 & Me: V2.0.0.0 (11/25/2003)
Driver Version for Win2K/XP: V2.0.0.7 (01/24/2003)
Driver Version for Win2K/XP: V2.0.0.8 (05/07/2003)

Files Included in This Release:
	DRemover.exe
	readme.txt
	serwpl.inf
	setup.exe
	Win98_ME\ser9pl.sys
	Win98_ME\serspl.inf
	Win98_ME\serspl.vxd
	Win2K_XP\pl2303.cat
	Win2K_XP\ser2pl.inf
	Win2K_XP\ser2pl.sys
			
Changes in this Release:
	1. For Windows2000 and XP: Bugfix regarding hardware handshake signals and other minor changes to increase 
		system stability. Passed MicroSoft Windows logo testing (WHQL).
	2. For Windows2000 and XP: Change of the driver version and date to V2.0.0.8, 05/07/2003.
	3. For Windows98 and ME: No change.
	4. Add 'setup.exe'.
	5. For Windows2000 and XP: Bugfix DCR value of PL2303, fix the problem of Pin23 always high at 5 voltage.

	
Note:   1. The USB-DC can only be used on a 500mA USB-Port. 
	   	Operation on a 100mA port may cause undesired results including system instability and loss of data.

	2. On WindowsXP: When install the driver to WinXP, must assign the path to "\Win2K_XP\ser2pl.inf".
		If you don't assign the correct path, the error will occur.
	
	3. After installation of the USB data cable driver and pluged-in data cable, a virtual COM port will be 
		generated. The name/ index of the allocated COM port can be accessed via the 'Device Manager'. 

	4. For deinstallation, after installation via 'setup.exe', please use the Control Panel - Add/Remove Program.

	5. After installation via Hardware Assistant the driver is not visible in the Control Panel. 
		Use for deinstallation the file 'DRemover.exe', stored on the driver CD.

	6. In case of any COM-port allocation conflict (e.g. with an onboard modem), 
		choose a higher COM port manually (e.g. above port 10) via 'Device Manager' for the USB data cable.

	7. Uninstall notice: If you install the driver by "setup.exe", before you uninstall the driver, 
		the USB data cable must plug into PC at least one time. If you don't follow this, the error may occur.
	

For FAQ and future updates of the USB device driver please visit the web: 
www.my-siemens.com

-------------------------------------------------------------------------------------------------------


Information sur ce release

Version de l'appl. (setup.exe) : V4.0.100 (04/15/2003)
Version de l'appl. (DRemover2K_XP.exe) : V1.3.0.1 (12/06/2002)
Version du pilote pour Win98 & Me : V2.0.0.0 (11/25/2003)
Version du pilote pour Win2K/XP: V2.0.0.7 (01/24/2003)

Fichiers inclus dans ce release :
	DRemover98_2K.exe
	readme.txt
	serwpl.inf
	setup.exe
	Win98_ME\ser9pl.sys
	Win98_ME\serspl.inf
	Win98_ME\serspl.vxd
	Win2K_XP\pl2303.cat
	Win2K_XP\ser2pl.inf
	Win2K_XP\ser2pl.sys
			
Changements de ce release :

	1. Pour Windows2000 et XP : Bugfix concernant les signaux d’établissement de liaison («handshake? 
		générés par le matériel et autres changements mineurs pour augmenter la stabilit?du système.
    		Test du logo MicroSoft Windows réussi (WHQL)
	2. Pour Windows2000 et XP : changement de la version de pilote et de la date en 
		V2.0.0.7, 01/24/2003 
	3. Pour Windows98 et Me : aucune modification

	
Rem. :  1. L'USB-DC peut uniquement s'utiliser sur un port USB 500mA. 	   	
		Toute utilisation sur un port 100mA peut provoquer des effets non désirés dont une instabilit?
                du système et des pertes de données.
	   		   
	2. Sous WindowsXP : l'installation via 'Setup.exe' n'est pas supportée. Utilisez l'Assistant Matériel pour 
		installer le pilote.
	
	3. Une fois l'installation du pilote du câble de données USB réalisée et le câble de données enfich? 
                un port COM virtuel est créé. Le nom/ index du port COM attribu?est visible dans le 'Gestionnaire de 					périphériques'. 

	4. Pour désinstaller un pilote install?avec 'setup.exe', utilisez le Panneau de configuration - 
                Ajout/Suppression de programmes.

	5. Après une installation avec l'Assistant Matériel, le pilote n'apparaît pas dans le Panneau de configuration. 
                Pour le désinstaller, utilisez le fichier 'DRemover98_2K.exe' sur le CD de pilotes.

	6. En cas de conflit d'attribution du port COM (par exemple avec un modem intégr?, 
		sélectionner pour le câble de données USB un port COM plus élev?(par exemple supérieur au port 10) 
		?l'aide du "Gestionnaire de périphériques".	

Pour vous informer sur les questions fréquentes (FAQ) et les futures mises ?jour du pilote du périphérique USB, 
visitez le site web ?l’adresse suivante: www.my-siemens.com

	
