Use WinSwup32.zip for XBI/XBZ-files for x35/x45-series

Use WinSwup_3.08.zip for XBZ-files for x5x-series:
A51, A52, A52M, A53, A56i, A57, A57A, SL55, SL5A, SL5E, ...

Use WinSwup_3.10.zip for XBZ-files for x60-series:
A60, A62, A62C, A65, A65C, C60, C60A, C61, CF62, CF6C, MC60, ...

You can download it at tools directory.

- Open correct WinSwup.
- You will get 'unknown error 0 occured', just click ok and ignore it.
- Goto file menu and select open.
- Open xbz-file.
- Software info will be read and phone can be flashed with it like with winswups including flash.

If you get 'No Update-SW found!': make sure you use correct winswup for xbz-file (just try the other one...).

If you get 'probably SGOLD-Sw loaded, not supported in WSWUP32, use SSWUP32 instead!': do not try to load x65/x70/x75 xbz-files, it will not work with these versions. Maybe one day a version for new series will work.


EH