Use WinSwup_4.18.zip for XBZ/XFS-files for SGOLD x65/x70/x75-series:
C65, C72, C75, CF75, CX65, CX70, CX75, M65, M75, ME75, S65, S68, SL65, SL75, ...

- Open WinSwup.
- Goto file menu and select open.
- Open xbz-file.
- Software info will be read and phone can be flashed with it like with winswups including flash.

If you get 'No Update-SW found!': make sure you are using WinSwup 4.18 and flashfile is correct/complete

If you get 'probably SGOLD-Sw loaded, not supported in WSWUP32, use SSWUP32 instead!': make sure you are using WinSwup_4.18

If you get 'Error old 24-Bit file: Please select a 32-Bit file for SGOLD': use Winswup 3.08 of 3.10 for EGOLD series

EH