MP4-19 TECHNICAL SPECIFICATION

Engine | Mercedes-Benz FO 110Q V10
Chassis | McLaren moulded carbon fibre/aluminium honeycomb composite incorporating front and side impact structures. Contains integral safety fuel cell
Front Suspension | Inboard torsion bar/damper system operated by pushrod and bell crank with a double wishbone arrangement
Rear Suspension | Inboard torsion bar/damper system operated by pushrod and bell crank with a double wishbone arrangement
Electronics | McLaren Electronic Systems control units incorporating electronics for chassis, engine and data acquisition. McLaren Electronic Systems also supplies the electronic dash board, alternator voltage control, sensors, data analysis and telemetry systems
Bodywork | Construction: One two-piece sidepod and engine cover. Separate floor section, structural nose with integral front wing
Tyres | Michelin
Race Wheels | Enkei
Fuel | Mobil Unleaded
Lubricants | Mobil 1 products
Adhesives | Henkel Technologies
Radios | Kenwood
Batteries | GS Battery

home