
  SiMoCo - Siemens Mobile Control 2.2.8
           S25, C35(i), M35, S35(i), SL42(i), SL45(i), C45, S45(i),
           ME45, M,MT50, C55, S55, SL55, M55, A60, C60, MC60, CF62,
           C65, M65, CX65, S65, CX70, C75, CX75, M75, S75 
  -------------------------------------------------------------------

  Software requierements: 32-bits operating system Windows
                          (95,98,ME,NT,2000,XP)

  Hardware requierements: mobile phone Siemens connected to computer
           either cable on serial port or over infra-red port, that
	   emulates the serial port COM (virtual infra COM port).


    Program properties:
    ------------------
  - displaying phone technical information
  - control of basic functions (call, hang up, volume, melody,
    vibrator, sound off, keyboard lock, handsfree)
  - indication of receiving call number, reply/reject of the call
  - displaying and editing of phonebooks (SIM, SIM fix, device) and
    addressbook, print, backup to file, restore from file, displaying
    all lists in one window with "drag and drop" potency, export/
    import VCARD in addressbook
  - writing and sending SMS with possibility of property editing -
    encoding, validity period, request status report, flash, long
    message (divide to max. 5 SMS)
  - multicast SMS (one SMS to a group), groups archiving
  - displaying and editing of SMS list in SIM and device memory
  - support of EMS standard (concatenated messages, predefined anima-
    tions and sounds, user animations and sounds, pictures). Sending
    and receiving of EMS messages is enabled also with MT, which hasn't
    this standard implemented (more in file EMS.txt)
  - automatic archiving of received and sent SMS, including EMS parts
  - export SMS to CSV file, saving of SMS text to file  
  - indication of new incoming SMS in a window or advice by a tray icon
  - access to flexmemory - file transfer between mobile and computer
  - displaying and editing of organiser with the daily schedule
  - full support of national characters (SMS and phonebooks UCS-2,
    addressbook and organiser UTF-8)
  - displaying of nets informations - available nets, preferred nets,
    operators, editing of preferred nets
  - sending of logo and screensaver from BMP or GIF file
  - delete logo and screensaver
  - logo editor
  - sending own melodies from MIDI files to max. 5 user positions
  - melody editor in iMELODY format, possible save melody as .txt (for
    archiving), iMELODY (for sending EMS) or MIDI (for uploading the
    own ringtone)
  - setting of call-forwarding and locking
  - synchronisation of MT date/time with computer date/time
  - sending of DTMF tones and strings (e.g. telebanking)
  - remote control of MT (emulation of the button pressing) - only if
    MT supports the command AT+CKPD
  - service menu activation (unwarranted - see history.txt)
  - possibility monitor the communication between program and phone in
    the terminal window, possibility own entering of the AT-commands

  Installation
  ------------
  To installation run program setup.exe. To uninstallation remove
  instalation folder from disk.

  If the program is used by more family members on the one computer, each
  of them must copy the runable program SiMoCo.exe and file Sx45DLL.dll
  to other (own) directory.  

  Most functions are placed in the "popup" menus, that are activated with
  the right mouse button - try everywhere press the right button. 

  License
  -------
  SiMoCo is freeware - free for copying and free for using.

  Author:  Ing. Pavel Cibulka, Na Pancave 591,
           538 51 Chrast u Chrudimi, CZ (Czech Republic) 
           cibulka.pavel@tiscali.cz

  -------------------------------------------------------------------------
     SiMoCo IS DISTRIBUTED "AS IS".  NO WARRANTY OF ANY
     KIND IS EXPRESSED OR IMPLIED.  YOU USE AT YOUR OWN RISK.
     THE AUTHOR WILL NOT BE LIABLE FOR DATA LOSS, DAMAGES, LOSS
     OF PROFITS OR ANY OTHER KIND OF LOSS WHILE USING OR MISUSING
     THIS SOFTWARE.
